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	BR 305 195
	PremiumLine self-draining eye shower with stainless steel bowl, floor mounted

	B-SAFETY PremiumLine self-draining eye shower with stainless steel bowl, floor mounted
- base plate with 4 mounting holes of stainless steel, polished, diameter 200 mm
- stand pipe 1 ¼” of stainless steel, polished, total height 1050 mm
- ball valve 1” of stainless steel, inclusive self-draining to the upper edge of the ball valve near the bottom, water inlet 1” male, DIN-DVGW tested and certificated
- Foot lever actuation made of plastic, total width 240 mm
- connection pipe of stainless steel for easy installation and alignment of the shower, polished
 - integrated flow regulation 14 litre / minute for a standard-compliant jet pattern at a specified working range of 2.5 to 5 bar flow pressure
- high-performance spray heads made of stainless steel for large-scale dispersion of water, with plastic spray plate, largely free of calcification, with rubber sleeves and sealed dust caps with folding mechanism, mounted over distributor fork
- bowl made of stainless steel, diameter 275 mm, polished, water outlet 1 ¼” male
- sign for eye shower according to EN ISO 7010 und ASR A1.3, self-adhesive PVC-film, 100 x 100 mm, viewing distance 10 metre
- total height 1050 mm, projection 375 mm, total width 275 mm
- according to BGI/GUV-I 850-0, DIN 1988 and EN 1717
- according to ANSI Z358.1-2014 and EN 15154-2:2006
- DIN-DVGW tested and certificated
Manufacturer: B-SAFETY or equal
Article-No.: BR 305 195

Technical Specifications
Minimum flow pressure: 2.5 bar
Operating pressure: 2.5 to 5 bar
Flow rate: 14 l/min
Water inlet: 1” male
Water outlet: 1 1/4” male
Dimensions (H x W x D): 1050 x 275 x 550 mm
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Safety showers for hot climates

www.b-safety.com
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